{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["12.9"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"12.9","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"merged":[[0,0,0,8],[16,0,16,7],[18,4,18,8]],"flags":["formulas_cached_only"]}
["四川财经职业学院第二学生食堂\n油烟净化器更换项目报价清单"]
[{"$nulls":8},"单位：人民币元"]
["序号","产品名称","规格(mm）","品牌","数量","单位","主要技术参数","单价/元","金额/元"]
[1,"油烟净化器","1180*900*820","重庆科旭",1,"台","外形尺寸：1180*900*820mm，进出风口尺寸800*1000mm，处理风量35000M3/H;阻力<150Pa；功率200W/220V；净化率>80%；投标人提供生产厂家加盖公章的“中国环境保护产品认证证书、高新产品技术证书及2017年同类产品的质量检测合格报告书”复印件。"]
[2,"净化器支架","1180*900*700","厂制品",1,"套","材质采用国标槽钢与∠40*40角钢制造，双层防腐处理；"]
[3,"出风口变径管","L*750*650","厂制品",1,"件","材质采用国标镀锌钢板制作,厚度1.0mm；内部压筋加强处理，烟管内连接处用玻璃硅胶密封。每件配角钢法兰盘1付，表面双层防腐处理。"]
[4,"出风口减振软联接","定制","厂制品",1,"件","烟管连接排风柜的接口，采用高级防雨水帆布制作。具有防震、防水、防火效果，减小风柜噪音。每件采用角钢法兰盘连接密封固定。"]
[5,"油烟净化器","1180*820*720","重庆科旭",1,"台","外形尺寸：1180*820*720mm，进出风口尺寸700*700mm，处理风量25000M3/H;阻力<150Pa；功率175W/220V。"]
[6,"净化器减震支架","1180*820*700","厂制品",1,"套","材质采用国标槽钢与∠40*40角钢制造，双层防腐处理。"]
[7,"风柜出风口变径管","L*670*600","厂制品",1,"件","材质采用国标镀锌钢板制作,厚度1.0mm；内部压筋加强处理，烟管内连接处用玻璃硅胶密封。每件配角钢法兰盘1付，表面双层防腐处理。"]
[8,"出风口减振软联接","定制","厂制品",1,"件","烟管连接排风柜的接口，采用高级防雨水帆布制作。具有防震、防水、防火效果，减小风柜噪音。每件采用角钢法兰盘连接密封固定。"]
[9,"弹簧减振器","配油烟净化器","成都振业",8,"只","阻尼型，减振效果好。"]
[10,"安装辅料",null,"厂制品",1,"项","含膨胀螺栓，吊钩、密封胶等。"]
[11,"旧设备拆除",null,"厂制品",1,"项"]
[12,"运输、装卸及搬运",null,"厂制品",1,"项"]
[13,"安装、调试",null,"厂制品",1,"项"]
["合计金额：",{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":4},"编制日期：2018 年 1 月 9 日"]