{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"merged":[[0,0,0,5],[4,0,5,0],[4,1,5,1],[4,5,5,5],[6,0,7,0],[6,1,7,1],[6,5,7,5],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,0,18,5]],"flags":["formulas_cached_only"]}
["财校会计技能国赛项目清单"]
["序号","设备名称","规格","数量","单位","备注"]
[1,"超五类线缆","CAT5E",22,"箱","大唐电信、TCL、飞利浦"]
[2,"强电线缆","BV4",1300,"米","熊猫、美河、三电"]
[3,"弱电线槽",70,200,"米","PVC抗压弧形线槽"]
[null,null,120,300,"米"]
[4,"强电线槽",50,200,"米","PVC抗压弧形线槽"]
[null,null,120,130,"米"]
[5,"机柜","1M600X600",8,"台","1米机柜（黑色、网孔门）图腾、跃图、华亿"]
[7,"插线板","3位3孔",88,"个","（公牛、子弹头、劳特）带开关、不带线"]
[8,"水晶头","超五类",10,"盒","同超五类线缆"]
[9,"比赛桌开孔","50mm",80,"张","每张桌开三孔，配塑料盖"]
[9,"地毯","2MM厚红色",1600,"平方"]
[10,"服务器机柜","42U",1,"台","\n1、标准:19英寸国际标准，高：2000(mm) 宽：600(mm) 深度1000(mm)，静载承重达1000KG\n2、门及门锁九折型材框架，方便拆卸的侧板和前后门，双钢质后门，\n3、材料及工艺主体采用承载能力强、耐腐蚀、易导电的优质型材为主体结构，配合优质冷扎钢板（主体2.0mm、架构2.0mm、防尘1.5mm）精工制作。\n4、机柜各部件或机柜表面脱脂、酸洗、磷化、静电喷塑。\n"]
[11,"　　辅　　材",null,1,"批"]
[12,"　　安装施工费",null,1,"项","线槽及强弱电施工"]
[13,"　　现场支持费",null,1,"项","２人２天"]
[14,"　　现场拆除费用",null,1,"项","拆除及搬运"]
["注：投标设备品牌必须为备注中品牌，以上报价为含税价，总预算78000元。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}