{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["1.15"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1.15","index":0,"n_rows":17,"n_cols":9,"rows_kept":17,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["四川财经职业学院第二学生食堂油烟净化器更换项目清单"]
[{"$nulls":8},"单位：人民币元"]
["序号","产品名称","品牌","型号、规格(mm）","数量","单位","主要技术参数或要求","单价/元","金额/元"]
[1,"油烟净化器","重庆添朗 ","KXU-YJ-40G",1,"台","进出风口尺寸1369*1676mm，处理风量35000M3/H;阻力<150Pa；功率4000W/220V；净化率≧80%；产品具有“中国环境保护产品认证证书、高新产品技术证书及2017年同类产品的质量检测合格报告书”。"]
[2,"净化器支架","厂制品","1180*900*700",1,"套","材质采用国标槽钢与∠40*40角钢制造，双层防腐处理；"]
[3,"出风口变径管","厂制品","L*750*650",1,"件","材质采用国标镀锌钢板制作,厚度1.0mm；内部压筋加强处理，烟管内连接处用玻璃硅胶密封。每件配角钢法兰盘1付，表面双层防腐处理。"]
[4,"出风口减振软联接","厂制品","定制",1,"件","烟管连接排风柜的接口，采用高级防雨水帆布制作。具有防震、防水、防火效果，减小风柜噪音。每件采用角钢法兰盘连接密封固定。"]
[5,"油烟净化器","重庆添朗 ","KXU-YJ-24G",1,"台","进出风口尺寸1369*1086mm，处理风量25000M3/H;阻力<150Pa；功率2400W/220V，净化率≧80%；产品具有“中国环境保护产品认证证书、高新产品技术证书及2017年同类产品的质量检测合格报告书”。"]
[6,"净化器减震支架","厂制品","1180*820*700",1,"套","材质采用国标槽钢与∠40*40角钢制造，双层防腐处理。"]
[7,"风柜出风口变径管","厂制品","L*670*600",1,"件","材质采用国标镀锌钢板制作,厚度1.0mm；内部压筋加强处理，烟管内连接处用玻璃硅胶密封。每件配角钢法兰盘1付，表面双层防腐处理。"]
[8,"出风口减振软联接","厂制品","定制",1,"件","烟管连接排风柜的接口，采用高级防雨水帆布制作。具有防震、防水、防火效果，减小风柜噪音。每件采用角钢法兰盘连接密封固定。"]
[9,"弹簧减振器","成都振业",null,8,"只","阻尼型，减振效果好（匹配相应的油烟净化器）。"]
[10,"安装辅料","厂制品",null,1,"项","含膨胀螺栓，吊钩、密封胶等。"]
[11,"旧设备拆除","厂制品",null,1,"项","搬运到指定的校内地点，规整放置"]
[12,"运输、装卸及搬运","厂制品",null,1,"项"]
[13,"安装、调试","厂制品",null,1,"项"]
[{"$nulls":7},"合计："]